In order to use analog displays in the Thermometer you must run Analogconfigurator.exe and
set and save all needed values. Remeber to give some name for the meter.
Suitable values for sample analogmeters:

                   Big meter                Small meter
-----------------------------------------------------------------------
Background image   bitmaps\back.bmp         bitmaps\back2.bmp
Mask image         bitmaps\mask.bmp         bitmaps\mask2.bmp
Needle length      80                       40
Needle width       3                        1
Max value          67                       67
Min value          -17                      -17
Max angle          9.0                      9
Min angle          260.0                    260
Origo X            113                      56
Origo Y            103                      51


See also the ReleaseNotes.txt.


If you start using this software please send a postcard (with a picture of your hometown) to 

Timo Sara-aho
Kopsantie 22
54110 Lampikangas
Finland
